Note, on all live electrical equipment where the work has been assessed as **HIGH** risk and above, this label is to be completed, attached and visible on the equipment prior to any live work commencing. After each break in work the label will need to be refreshed.

**Familiar with circuit & component location**

**Equipment**

**(Under Test)**

**Date**

**Competent**

**Person**

**Tick**

**Environment is Safe:**

**Clear escape route identified**

**Barriers & warning signs in place**

**Personal safety equipment worn**

**Tools & Test equipment insulated**

**Equipment knowledge:**

**Safety Observer ready:**

**Power isolation identified**

**Trained in isolating this equipment**

**Free of all other duties**

**Name:**

**Working on Live Equipment Checklist**

**ANU**

**(before starting work)**

**Safe Work Procedures available:**

**Safe Work Method Statement**

**Safe Operating Procedure**