# GAS LEAK

It is important to know what you are handling in the first place. Only those people trained in the storage and handling of dangerous goods should have access to them.

* Assist persons in immediate danger immediately (only if safe to do so);
* If flammable – shut off all ignition sources (only if safe to do so);
* Raise the alarm – Notify Fire Brigade on **0-000** and give details of problem;
* Alert ANU Security on extension **52249** or phone **(02) 6125 2249;**
* Evacuate to the designated emergency assembly area. **DO NOT** return to the building until advised to do so by the Building Chief Warden or Emergency Services; and
* Remove any personnel from the vicinity of the area downwind of the gas leak.

*An alternative emergency assembly area may need to be used if the weather conditions are transporting vapours toward the primary assembly area. Listen for instructions and take note of unusual smells and conditions.*

More safety information is available through online learning modules in [Pulse.](https://anu.interactiontraining.net/Central/) Search for chemical safety courses on gas cylinders, and cryogenic materials.