### Laboratory and Fume Exhaust System Details

|  |  |
| --- | --- |
| **Laboratory** |       |
| **Laboratory Supervisor** |       |
| **Telephone** |       |
| **Fume Cupboard Number** |       |
| **Scrubbed Cupboard** |       |
| Operating guide -pH range 6.5 – 9Dosing chemical – Sodium hydroxide pellets (10g / Tank)pH to be checked regularly (monthly minimum), under current usageConsult the procedure attached to the inside of the back cover. |

### Fume Exhaust System Log (page in book or loose leaf sheets in a folder)

| **Date** | **Name** | **Maintenance or Repair Conducted** | **Comment** | **Operation Satisfactory? (Yes/No)** |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |